EE 4743 –T est 2 – Fall 1998

1 Sam Russ

T est #2 – EE 4743 – Fall 1998 My Name is: _____________________________

Y ou have 50 minutes to complete this test. Good luck!

1. (15) Answer the following short questions.

a. Y ou are a middle–level manager. One of your employees has fully pipelined a flowgraph

(down to 1 clock cycle per sample period). He tells you that it will take him three days to

design the control unit for the flowgraph. What is wrong with that?

b. Fill in the blanks:

Pipelining increases _____________________________________ but makes

______________________________________ worse.

c. Name two techniques that may let you reduce the critical path without increasing latency.

EE 4743 –T est 2 – Fall 1998

2 Sam Russ

2. (30 points) Consider the equation below.

Y = 0.5 Y@1 + 0.75 X – X@1

a. Convert the equation to ‘‘shift–and–add’ ’ format.

b. Draw a flowgraph for it. Assume shifts are combinational. Don’t worry about minimizing

anything!

c. What is the critical path? __________ The iteration loop critical path? __________

d. Assume that the number of clock cycles per sample period equals the critical path. Estimate

the amount of resources needed based on the total number of shifts and adds that are per-

formed and the number of clock cycles.

Number of Adders: __________ Number of Shifters: __________

e. Assign TASAP and TALAP pairs to the flowgraph. (Hint: You may want to redraw the graph

below .)

EE 4743 –T est 2 – Fall 1998

3 Sam Russ f. Schedule the flowgraph. Do not worry about amount of resources (for example, number of

registers).

EE 4743 –T est 2 – Fall 1998

4 Sam Russ

3. (35 points) Consider the schedule below.

CC Adder Shifter A B C D E

0 A >> 2 Ld Shifter ///// ///// Load X

1 D >> 1 ///// ///// ///// Ld. Shifter

2 A + E C >> 3 Ld. Shifter ///// Ld. Adder /////

3 A + C ///// Ld. Adder /////

3 B + C;

output is Y

Ld. Adder Load D Load B

a. Use the schedule to reconstruct the original flowgraph.

b. Use the flowgraph to reconstruct the original equation.

EE 4743 –T est 2 – Fall 1998

5 Sam Russ c. Redraw the flowgraph to minimize the iteration loop critical path. For full credit, your flow-

graph should have the minimum critical path that is acheivable once the iteration loop critical

path has been minimized. ONLY REDRAW the flowgraph; don’t pipeline it!

EE 4743 –T est 2 – Fall 1998

6 Sam Russ

4. (20 points) Consider the diagrams and answer the questions below. Note that the flip flop is drawn

‘ ‘backwards’ ’.

P_state

N_state

X

L

D Q

Clk

DFF0

Clk

7 ns

8ns

2 ns

3 ns t

S U

= 4 ns

t

H D

= 5 ns

t

C Q

= 6 ns

a. (10) What are the external setup and hold times for input X? Hint:

DIN t

S U

= DFF t

S U

+ DIN t

P D max – Clk t

P D min

DIN t

H D

= DFF t

H D

– DIN t

P D min + Clk t

P D max

X to DFF0: Setup Time: Hold Time:

b. (10) What is the delay from the clock to output L?

Delay from Clk to L:

c. (10) What is the clock cycle time based on register–to–register delays?

Register–to–Register Clock Cycle Time: